**Date Issued: September 22, 2017**

**Rinex v1.9.3**

|  |
| --- |
| **Update** |
| Correction to “Data Rate” configuration handling in Rinex Desktop |
| Improves BDS ephemeris timestamp output |
| Improves start/stop marker messages handling |

**Rinex v1.9.2**

|  |
| --- |
| **Update** |
| Improvements to automatic interval detection |

**Rinex v1.9.1**

|  |
| --- |
| **Update** |
| For RinexSLX when interval is unspecified, all observations will be output |
| Correctly handle user-specified observation intervals |

*We thank you for your continued business. Please contact your Hemisphere GNSS technical support representative with any additional questions.*

This document is provided for technical support purposes only. Please refer to the product documentation for warranty, license and safety information associated with the product.